105206

(DRIVING E TO W)

1.	LT AND RT (TYPE A) - REPLACE 
2.	28" AT BRIDGE, REST GOOD - DBR
3.	HEIGHT GOOD ON BRIDGE BUT SHORT OFF BRIDGE SECTIONS; STEEL GAP FOR EXPANSION JOINT STILL 2.5" - REPLACE ALL AND DBR
4.	ALL GOOD (WELL ABOVE 26.5") - GOOD
5.	NEAR END IS 27.5", ALL ELSE IS TALLER - GOOD