107602

(DRIVING N TO S)

1.	RT BEFORE RR TYPE E DAMAGED & GR LOW. AFTER RR LOW AS WELL. REPLACE. ---DONE
2.	TYPE A BOTH ENDS. REPLACE. ---DONE
3.	CURVED END AT DRIVE IS LOW. REST GOOD. CHECK IF GUARDRAIL IS SUFFICIENT AT RETAINING WALL. - LEAVE OUT OF PROJECT (OUTSIDE SCOPE)

(DRIVING S TO N)

4.	SLIGHTLY LOW THROUGHOUT (AT NORTHSTAR CENTER). REPLACE.
5.	SLIGHTLY LOW THROUGHOUT (ENDS AREN'T TYPE E. CHECK WITH GARRETT ABOUT THE END TREATMENT BETWEEN RR AND BRIDGE) ---RAILROAD
