# Survey Report

Job name | ODOT D11 culverts
Creation date | 16 Dec 2025
Version | Trimble Access 22.10
Distance Units | US survey feet
Angle units | Degrees
Pressure Units | inHg
Temperature Units | Fahrenheit

Coordinate system (Job)

System | United States/NAD83
Zone | Ohio North 3401
Datum | NAD83(2011)

Projection

Projection | Lambert Conformal Conic 2 Parallel
Origin lat | 39°40'00.00000"N
Origin long | 82°30'00.00000"W
False northing | 0.000
False easting | 1968500.000
Parallel 1 | 41°42'00.00000"N
Parallel 2 | 40°26'00.00000"N
South azimuth (grid) | No
Grid coords | Increase North-East
Ellipsoid | Semi-major axis: 20925604.474 Flattening: 298.25722210

Local site

Type | Grid

Datum transformation

Type | Three parameter
Semi-major axis | 20925604.474
Flattening | 298.257223
Translation X | 0.000
Translation Y | 0.000
Translation Z | 0.000

Vertical adjustment

Geoid file | GEOID18 (Conus) Fixed

Collected Field Data (ECEF deltas: APC to APC)

Corrections

South azimuth (grid) | No
Grid coords | Increase North-East
Magnetic declination | 0°00'00"
Distances | Ground
Neighborhood adjustment | Off

Projection

Projection | Lambert Conformal Conic 2 Parallel
Origin lat | 39°40'00.00000"N
Origin long | 82°30'00.00000"W
False northing | 0.000
False easting | 1968500.000
Parallel 1 | 41°42'00.00000"N
Parallel 2 | 40°26'00.00000"N
Ellipsoid | Semi-major axis: 20925604.474 Flattening: 298.25722210

Local site

Type | Grid

Datum transformation

Type | Three parameter
Semi-major axis | 20925604.474
Flattening | 298.257223
Translation X | 0.000
Translation Y | 0.000
Translation Z | 0.000

Vertical adjustment

Geoid file | GEOID18 (Conus) Fixed

Coordinate system

System | United States/NAD83
Zone | Ohio North 3401
Datum | NAD83(2011)

Feature library

Library name | ODOT_SurveyCodes
Library File Name | ODOT_SurveyCodes.fxl
Attribute Support | Yes

Point | 5001 | North | 258014.023 | East | 2382495.544 | Elevation | 1016.207 | Code | CNPT-A

Point | 5002 | North | 257882.826 | East | 2382262.423 | Elevation | 1009.484 | Code | CNPT-B

Point | 5003 | North | 257882.862 | East | 2382262.434 | Elevation | 1009.490 | Code | CNPT-B

Point | 5004 | North | 257882.850 | East | 2382262.410 | Elevation | 1009.513 | Code | CNPT-B

Point | 5005 | North | 257882.855 | East | 2382262.411 | Elevation | 1009.496 | Code | CNPT-B

Point | 5006 | North | 257859.556 | East | 2381972.793 | Elevation | 1002.834 | Code | CNPT-C

Point | 5007 | North | 257859.560 | East | 2381972.768 | Elevation | 1002.842 | Code | CNPT-C

Point | 5008 | North | 257859.607 | East | 2381972.782 | Elevation | 1002.819 | Code | CNPT-C

Point | 5009 | North | 257859.609 | East | 2381972.762 | Elevation | 1002.810 | Code | CNPT-C

Point | 5010 | North | 258014.060 | East | 2382495.589 | Elevation | 1016.251 | Code | CNPT-A

Point | 5011 | North | 258014.082 | East | 2382495.597 | Elevation | 1016.243 | Code | CNPT-A

Point | 5012 | North | 258014.079 | East | 2382495.569 | Elevation | 1016.238 | Code | CNPT-A

Point | 5013 | North | 253509.984 | East | 2377920.883 | Elevation | 1144.999 | Code | CNPT-D

Point | 5014 | North | 253509.975 | East | 2377920.939 | Elevation | 1144.992 | Code | CNPT-D

Point | 5015 | North | 253509.973 | East | 2377920.917 | Elevation | 1145.082 | Code | CNPT-D

Point | 5016 | North | 253509.968 | East | 2377920.885 | Elevation | 1145.123 | Code | CNPT-D

Point | 5017 | North | 253498.000 | East | 2377962.746 | Elevation | 1144.597 | Code | CNPT-E

Point | 5018 | North | 253498.024 | East | 2377962.721 | Elevation | 1144.595 | Code | CNPT-E

Point | 5019 | North | 253498.016 | East | 2377962.777 | Elevation | 1144.534 | Code | CNPT-E

Point | 5020 | North | 253498.010 | East | 2377962.754 | Elevation | 1144.605 | Code | CNPT-E

Point | 5021 | North | 253829.595 | East | 2377972.687 | Elevation | 1132.795 | Code | CNPT-F

Point | 5022 | North | 253829.601 | East | 2377972.662 | Elevation | 1132.800 | Code | CNPT-F

Point | 5023 | North | 253829.572 | East | 2377972.700 | Elevation | 1132.834 | Code | CNPT-F

Point | 5024 | North | 253829.608 | East | 2377972.708 | Elevation | 1132.781 | Code | CNPT-F

Point | 5025 | North | 185451.446 | East | 2392765.419 | Elevation | 1051.787 | Code | CNPT-G

Point | 5026 | North | 185451.461 | East | 2392765.426 | Elevation | 1051.786 | Code | CNPT-G

Point | 5027 | North | 185451.455 | East | 2392765.430 | Elevation | 1051.765 | Code | CNPT-G

Point | 5028 | North | 185451.471 | East | 2392765.399 | Elevation | 1051.753 | Code | CNPT-G

Rover options

Elevation mask | 10 | PDOP mask | 6 |  |  |  |  |  |

Rover options

Elevation mask | 10 | PDOP mask | 6 |  |  |  |  |  |

Survey event

Survey event | Rover started

Point | PRS33667490340 | Latitude | 40°12'05.96943"N | Longitude | 81°15'28.22083"W | Height | 901.177 | Code |

GNSS receiver

Receiver type | Unknown
Serial number |
Firmware version | 0
Antenna type | AdV Null Antenna
Measurement method | Antenna Phase Center
Tape adjustment | 0.000
Horizontal offset | 0.000
Vertical offset | 0.000

Base point

Point | PRS33667490340 | Antenna height | 0.000 | Type | Corrected |  |  |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 224519 | Initialization type | On the fly | Survey type | Real-time |  |

GNSS receiver

Receiver type | R12i
Serial number | 6212F02057
Firmware version | 6.14
Antenna type | R12i Internal
Measurement method | Bottom of quick release
Tape adjustment | 0.000
Horizontal offset | 0.000
Vertical offset | 0.588

Point | 1000 | ΔX | 57113.994 | ΔY | 44864.991 | ΔZ | 42154.591 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.060 | Vt Prec (1 sigma) | 0.097 |  |
QC 1 |  | PDOP | 1.3 | GDOP | 1.9 | HDOP | 0.7 | VDOP | 1.0
|  | Base data age | 1 | Positions used | 55 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 25, 26, 28, 31, 32
Satellites: (GLONASS) | 4, 12, 14
Satellites: (GALILEO) | 10, 12, 19, 21, 27, 29

QC 2 |  | VCV xx (m²) | 0.000131 | VCV xy (m²) | -0.000015 | VCV xz (m²) | 0.000051 |  |
|  |  |  | VCV yy (m²) | 0.000660 | VCV yz (m²) | -0.000320 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000419 |  |

Feature (1000) | CMON
Depth |
Note | E

Point | 1001 | ΔX | 57114.015 | ΔY | 44864.904 | ΔZ | 42154.657 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.086 | Vt Prec (1 sigma) | 0.142 |  |
QC 1 |  | PDOP | 1.2 | GDOP | 1.9 | HDOP | 0.7 | VDOP | 1.0
|  | Base data age | 1 | Positions used | 31 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 25, 26, 28, 29, 31, 32
Satellites: (GLONASS) | 2, 4, 14
Satellites: (GALILEO) | 10, 12, 19, 21, 27, 29

QC 2 |  | VCV xx (m²) | 0.000249 | VCV xy (m²) | 0.000325 | VCV xz (m²) | -0.000109 |  |
|  |  |  | VCV yy (m²) | 0.001622 | VCV yz (m²) | -0.000757 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000681 |  |

Warnings (1001) | Poor precision

Feature (1001) | CMON
Depth |
Note | E

Point | 1002 | ΔX | 57114.087 | ΔY | 44864.975 | ΔZ | 42154.597 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.082 | Vt Prec (1 sigma) | 0.128 |  |
QC 1 |  | PDOP | 1.3 | GDOP | 2.1 | HDOP | 0.7 | VDOP | 1.1
|  | Base data age | 1 | Positions used | 41 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 25, 26, 28, 31, 32
Satellites: (GLONASS) | 4, 14
Satellites: (GALILEO) | 4, 10, 12, 19, 21, 27, 29

QC 2 |  | VCV xx (m²) | 0.000235 | VCV xy (m²) | 0.000164 | VCV xz (m²) | -0.000075 |  |
|  |  |  | VCV yy (m²) | 0.001199 | VCV yz (m²) | -0.000590 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000706 |  |

Warnings (1002) | Poor precision

Feature (1002) | CMON
Depth |
Note | E

Point | 1003 | ΔX | 57114.069 | ΔY | 44865.010 | ΔZ | 42154.596 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.081 | Vt Prec (1 sigma) | 0.127 |  |
QC 1 |  | PDOP | 1.6 | GDOP | 2.5 | HDOP | 0.9 | VDOP | 1.3
|  | Base data age | 1 | Positions used | 32 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 31, 32
Satellites: (GLONASS) | 4, 14
Satellites: (GALILEO) | 4, 10, 12, 19, 21, 27, 29

QC 2 |  | VCV xx (m²) | 0.000209 | VCV xy (m²) | 0.000138 | VCV xz (m²) | -0.000044 |  |
|  |  |  | VCV yy (m²) | 0.001233 | VCV yz (m²) | -0.000569 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000672 |  |

Feature (1003) | CMON
Depth |
Note | E

Point | 1004 | ΔX | 57071.687 | ΔY | 44866.310 | ΔZ | 42164.473 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.062 | Vt Prec (1 sigma) | 0.080 |  |
QC 1 |  | PDOP | 1.1 | GDOP | 1.6 | HDOP | 0.7 | VDOP | 0.8
|  | Base data age | 1 | Positions used | 42 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 25, 26, 28, 29, 31, 32
Satellites: (GLONASS) | 2, 4, 14
Satellites: (GALILEO) | 10, 12, 19, 21, 27, 29

QC 2 |  | VCV xx (m²) | 0.000140 | VCV xy (m²) | 0.000008 | VCV xz (m²) | 0.000020 |  |
|  |  |  | VCV yy (m²) | 0.000451 | VCV yz (m²) | -0.000191 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000355 |  |

Feature (1004) | CMON
Depth |
Note | D

Point | 1005 | ΔX | 57071.645 | ΔY | 44866.331 | ΔZ | 42164.501 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.066 | Vt Prec (1 sigma) | 0.093 |  |
QC 1 |  | PDOP | 1.3 | GDOP | 2.0 | HDOP | 0.7 | VDOP | 1.1
|  | Base data age | 1 | Positions used | 32 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 25, 26, 28, 29, 31, 32
Satellites: (GLONASS) | 2, 4, 14
Satellites: (GALILEO) | 4, 10, 12, 19, 21, 27, 29

QC 2 |  | VCV xx (m²) | 0.000170 | VCV xy (m²) | 0.000014 | VCV xz (m²) | 0.000042 |  |
|  |  |  | VCV yy (m²) | 0.000590 | VCV yz (m²) | -0.000280 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000447 |  |

Feature (1005) | CMON
Depth |
Note | D

Point | 1006 | ΔX | 57071.577 | ΔY | 44866.303 | ΔZ | 42164.526 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.064 | Vt Prec (1 sigma) | 0.088 |  |
QC 1 |  | PDOP | 1.2 | GDOP | 1.9 | HDOP | 0.7 | VDOP | 0.9
|  | Base data age | 1 | Positions used | 31 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 25, 26, 28, 29, 31, 32
Satellites: (GLONASS) | 4, 14
Satellites: (GALILEO) | 4, 10, 12, 19, 21, 27, 29

QC 2 |  | VCV xx (m²) | 0.000152 | VCV xy (m²) | 0.000039 | VCV xz (m²) | 0.000029 |  |
|  |  |  | VCV yy (m²) | 0.000531 | VCV yz (m²) | -0.000254 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000422 |  |

Feature (1006) | CMON
Depth |
Note | D

Point | 1007 | ΔX | 57071.577 | ΔY | 44866.311 | ΔZ | 42164.472 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.067 | Vt Prec (1 sigma) | 0.088 |  |
QC 1 |  | PDOP | 1.3 | GDOP | 2.0 | HDOP | 0.8 | VDOP | 1.0
|  | Base data age | 1 | Positions used | 31 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 29, 31, 32
Satellites: (GLONASS) | 4, 14
Satellites: (GALILEO) | 4, 10, 12, 19, 21, 23, 27, 29

QC 2 |  | VCV xx (m²) | 0.000160 | VCV xy (m²) | 0.000028 | VCV xz (m²) | 0.000044 |  |
|  |  |  | VCV yy (m²) | 0.000526 | VCV yz (m²) | -0.000239 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000458 |  |

Feature (1007) | CMON
Depth |
Note | D

Point | 1008 | ΔX | 57094.482 | ΔY | 45088.204 | ΔZ | 42399.463 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.068 | Vt Prec (1 sigma) | 0.096 |  |
QC 1 |  | PDOP | 1.4 | GDOP | 2.1 | HDOP | 0.8 | VDOP | 1.1
|  | Base data age | 1 | Positions used | 32 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 31, 32
Satellites: (GLONASS) | 4, 14, 15
Satellites: (GALILEO) | 4, 10, 12, 19, 21, 23, 27, 29

QC 2 |  | VCV xx (m²) | 0.000150 | VCV xy (m²) | 0.000058 | VCV xz (m²) | 0.000008 |  |
|  |  |  | VCV yy (m²) | 0.000689 | VCV yz (m²) | -0.000296 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000446 |  |

Feature (1008) | CMON
Depth |
Note | F

Point | 1009 | ΔX | 57094.555 | ΔY | 45088.223 | ΔZ | 42399.441 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.060 | Vt Prec (1 sigma) | 0.087 |  |
QC 1 |  | PDOP | 1.2 | GDOP | 1.8 | HDOP | 0.7 | VDOP | 1.0
|  | Base data age | 1 | Positions used | 32 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 31, 32
Satellites: (GLONASS) | 2, 4, 14, 15
Satellites: (GALILEO) | 4, 10, 12, 19, 21, 23, 27, 29

QC 2 |  | VCV xx (m²) | 0.000131 | VCV xy (m²) | 0.000011 | VCV xz (m²) | 0.000036 |  |
|  |  |  | VCV yy (m²) | 0.000538 | VCV yz (m²) | -0.000249 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000371 |  |

Feature (1009) | CMON
Depth |
Note | F

Point | 1010 | ΔX | 57094.601 | ΔY | 45088.300 | ΔZ | 42399.399 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.054 | Vt Prec (1 sigma) | 0.073 |  |
QC 1 |  | PDOP | 1.2 | GDOP | 1.8 | HDOP | 0.7 | VDOP | 1.0
|  | Base data age | 1 | Positions used | 33 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 31, 32
Satellites: (GLONASS) | 2, 4, 14, 15
Satellites: (GALILEO) | 4, 10, 19, 21, 23, 27, 29

QC 2 |  | VCV xx (m²) | 0.000106 | VCV xy (m²) | 0.000022 | VCV xz (m²) | 0.000022 |  |
|  |  |  | VCV yy (m²) | 0.000409 | VCV yz (m²) | -0.000160 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000251 |  |

Feature (1010) | CMON
Depth |
Note | F

Point | 1011 | ΔX | 57094.548 | ΔY | 45088.261 | ΔZ | 42399.406 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.056 | Vt Prec (1 sigma) | 0.077 |  |
QC 1 |  | PDOP | 1.2 | GDOP | 1.8 | HDOP | 0.7 | VDOP | 1.0
|  | Base data age | 1 | Positions used | 32 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 31, 32
Satellites: (GLONASS) | 2, 4, 14, 15
Satellites: (GALILEO) | 4, 10, 12, 19, 21, 23, 27, 29

QC 2 |  | VCV xx (m²) | 0.000121 | VCV xy (m²) | 0.000018 | VCV xz (m²) | 0.000020 |  |
|  |  |  | VCV yy (m²) | 0.000466 | VCV yz (m²) | -0.000181 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000245 |  |

Feature (1011) | CMON
Depth |
Note | F

Initialization event: RTK not initialized

GPS week | 2397 | Seconds | 226775 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 226777 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK not initialized

GPS week | 2397 | Seconds | 230690 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 230706 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK not initialized

GPS week | 2397 | Seconds | 230983 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 230998 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK not initialized

GPS week | 2397 | Seconds | 231898 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 231900 | Initialization type | On the fly | Survey type | Real-time |  |

Point | 1012 | ΔX | 61202.565 | ΔY | 48519.975 | ΔZ | 45453.795 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.031 | Vt Prec (1 sigma) | 0.041 |  |
QC 1 |  | PDOP | 1.3 | GDOP | 2.4 | HDOP | 0.7 | VDOP | 1.1
|  | Base data age | 1 | Positions used | 34 |  |  |  |

Satellites: (GPS) | 3, 4, 9, 16, 26, 28, 31
Satellites: (GLONASS) | 4, 5, 14, 15
Satellites: (GALILEO) | 4, 6, 19, 21, 23, 27, 29
Satellites: (BEIDOU) | 11

QC 2 |  | VCV xx (m²) | 0.000034 | VCV xy (m²) | 0.000001 | VCV xz (m²) | 0.000009 |  |
|  |  |  | VCV yy (m²) | 0.000076 | VCV yz (m²) | -0.000056 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000138 |  |

Feature (1012) | CMON
Depth |
Note | A

Point | 1013 | ΔX | 61202.578 | ΔY | 48519.999 | ΔZ | 45453.823 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.028 | Vt Prec (1 sigma) | 0.036 |  |
QC 1 |  | PDOP | 1.3 | GDOP | 2.4 | HDOP | 0.7 | VDOP | 1.1
|  | Base data age | 1 | Positions used | 41 |  |  |  |

Satellites: (GPS) | 3, 4, 9, 16, 26, 28, 31
Satellites: (GLONASS) | 4, 5, 14, 15
Satellites: (GALILEO) | 4, 6, 19, 21, 23, 27, 29
Satellites: (BEIDOU) | 11

QC 2 |  | VCV xx (m²) | 0.000028 | VCV xy (m²) | -0.000001 | VCV xz (m²) | 0.000006 |  |
|  |  |  | VCV yy (m²) | 0.000064 | VCV yz (m²) | -0.000043 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000102 |  |

Feature (1013) | CMON
Depth |
Note | A

Point | 1014 | ΔX | 61202.540 | ΔY | 48520.025 | ΔZ | 45453.803 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.027 | Vt Prec (1 sigma) | 0.036 |  |
QC 1 |  | PDOP | 1.3 | GDOP | 2.4 | HDOP | 0.7 | VDOP | 1.1
|  | Base data age | 1 | Positions used | 32 |  |  |  |

Satellites: (GPS) | 3, 4, 9, 16, 26, 28, 31
Satellites: (GLONASS) | 4, 5, 14, 15
Satellites: (GALILEO) | 4, 6, 19, 21, 23, 27, 29
Satellites: (BEIDOU) | 11

QC 2 |  | VCV xx (m²) | 0.000026 | VCV xy (m²) | -0.000002 | VCV xz (m²) | 0.000003 |  |
|  |  |  | VCV yy (m²) | 0.000062 | VCV yz (m²) | -0.000043 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000096 |  |

Feature (1014) | CMON
Depth |
Note | A

Point | 1015 | ΔX | 61202.510 | ΔY | 48519.998 | ΔZ | 45453.795 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.025 | Vt Prec (1 sigma) | 0.034 |  |
QC 1 |  | PDOP | 1.3 | GDOP | 2.4 | HDOP | 0.7 | VDOP | 1.1
|  | Base data age | 1 | Positions used | 43 |  |  |  |

Satellites: (GPS) | 3, 4, 9, 16, 26, 28, 31
Satellites: (GLONASS) | 4, 5, 14, 15
Satellites: (GALILEO) | 4, 6, 19, 21, 23, 27, 29
Satellites: (BEIDOU) | 11

QC 2 |  | VCV xx (m²) | 0.000024 | VCV xy (m²) | -0.000002 | VCV xz (m²) | 0.000002 |  |
|  |  |  | VCV yy (m²) | 0.000060 | VCV yz (m²) | -0.000038 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000080 |  |

Feature (1015) | CMON
Depth |
Note | A

Point | 1016 | ΔX | 60982.133 | ΔY | 48406.980 | ΔZ | 45352.429 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.026 | Vt Prec (1 sigma) | 0.034 |  |
QC 1 |  | PDOP | 1.3 | GDOP | 2.3 | HDOP | 0.7 | VDOP | 1.1
|  | Base data age | 1 | Positions used | 44 |  |  |  |

Satellites: (GPS) | 3, 4, 9, 16, 26, 28, 31
Satellites: (GLONASS) | 4, 5, 14, 15
Satellites: (GALILEO) | 4, 6, 19, 21, 23, 27, 29
Satellites: (BEIDOU) | 11

QC 2 |  | VCV xx (m²) | 0.000025 | VCV xy (m²) | -0.000002 | VCV xz (m²) | 0.000005 |  |
|  |  |  | VCV yy (m²) | 0.000058 | VCV yz (m²) | -0.000038 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000085 |  |

Feature (1016) | CMON
Depth |
Note | B

Point | 1017 | ΔX | 60982.129 | ΔY | 48406.976 | ΔZ | 45352.407 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.024 | Vt Prec (1 sigma) | 0.032 |  |
QC 1 |  | PDOP | 1.3 | GDOP | 2.3 | HDOP | 0.7 | VDOP | 1.1
|  | Base data age | 1 | Positions used | 32 |  |  |  |

Satellites: (GPS) | 3, 4, 9, 16, 26, 28, 31
Satellites: (GLONASS) | 4, 5, 14, 15
Satellites: (GALILEO) | 4, 6, 19, 21, 23, 27, 29
Satellites: (BEIDOU) | 11

QC 2 |  | VCV xx (m²) | 0.000022 | VCV xy (m²) | -0.000002 | VCV xz (m²) | 0.000006 |  |
|  |  |  | VCV yy (m²) | 0.000053 | VCV yz (m²) | -0.000034 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000075 |  |

Feature (1017) | CMON
Depth |
Note | B

Point | 1018 | ΔX | 60982.145 | ΔY | 48406.994 | ΔZ | 45352.377 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.024 | Vt Prec (1 sigma) | 0.032 |  |
QC 1 |  | PDOP | 1.3 | GDOP | 2.3 | HDOP | 0.8 | VDOP | 1.1
|  | Base data age | 1 | Positions used | 33 |  |  |  |

Satellites: (GPS) | 3, 4, 9, 16, 26, 28, 31
Satellites: (GLONASS) | 4, 5, 14, 15
Satellites: (GALILEO) | 4, 6, 19, 21, 23, 27, 29
Satellites: (BEIDOU) | 11

QC 2 |  | VCV xx (m²) | 0.000022 | VCV xy (m²) | -0.000001 | VCV xz (m²) | 0.000007 |  |
|  |  |  | VCV yy (m²) | 0.000054 | VCV yz (m²) | -0.000034 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000074 |  |

Feature (1018) | CMON
Depth |
Note | B

Point | 1019 | ΔX | 60982.160 | ΔY | 48407.015 | ΔZ | 45352.390 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.023 | Vt Prec (1 sigma) | 0.032 |  |
QC 1 |  | PDOP | 1.3 | GDOP | 2.3 | HDOP | 0.7 | VDOP | 1.1
|  | Base data age | 1 | Positions used | 32 |  |  |  |

Satellites: (GPS) | 3, 4, 9, 16, 26, 28, 31
Satellites: (GLONASS) | 4, 5, 14, 15
Satellites: (GALILEO) | 4, 6, 19, 21, 23, 27, 29
Satellites: (BEIDOU) | 11

QC 2 |  | VCV xx (m²) | 0.000021 | VCV xy (m²) | 0.000000 | VCV xz (m²) | 0.000005 |  |
|  |  |  | VCV yy (m²) | 0.000054 | VCV yz (m²) | -0.000033 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000069 |  |

Feature (1019) | CMON
Depth |
Note | B

Point | 1020 | ΔX | 60696.754 | ΔY | 48354.940 | ΔZ | 45334.161 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.025 | Vt Prec (1 sigma) | 0.032 |  |
QC 1 |  | PDOP | 1.3 | GDOP | 2.3 | HDOP | 0.7 | VDOP | 1.1
|  | Base data age | 1 | Positions used | 41 |  |  |  |

Satellites: (GPS) | 3, 4, 9, 16, 26, 28, 31
Satellites: (GLONASS) | 4, 5, 14, 15
Satellites: (GALILEO) | 4, 6, 19, 21, 23, 27, 29
Satellites: (BEIDOU) | 11

QC 2 |  | VCV xx (m²) | 0.000023 | VCV xy (m²) | -0.000001 | VCV xz (m²) | 0.000008 |  |
|  |  |  | VCV yy (m²) | 0.000053 | VCV yz (m²) | -0.000032 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000076 |  |

Feature (1020) | CMON
Depth |
Note | C

Point | 1021 | ΔX | 60696.729 | ΔY | 48354.924 | ΔZ | 45334.145 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.025 | Vt Prec (1 sigma) | 0.032 |  |
QC 1 |  | PDOP | 1.3 | GDOP | 2.3 | HDOP | 0.7 | VDOP | 1.0
|  | Base data age | 1 | Positions used | 31 |  |  |  |

Satellites: (GPS) | 3, 4, 8, 9, 16, 26, 28, 31
Satellites: (GLONASS) | 4, 5, 14, 15
Satellites: (GALILEO) | 4, 6, 19, 21, 23, 27, 29
Satellites: (BEIDOU) | 11

QC 2 |  | VCV xx (m²) | 0.000023 | VCV xy (m²) | -0.000001 | VCV xz (m²) | 0.000007 |  |
|  |  |  | VCV yy (m²) | 0.000053 | VCV yz (m²) | -0.000033 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000076 |  |

Feature (1021) | CMON
Depth |
Note | C

Point | 1022 | ΔX | 60696.740 | ΔY | 48354.917 | ΔZ | 45334.132 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.025 | Vt Prec (1 sigma) | 0.033 |  |
QC 1 |  | PDOP | 1.2 | GDOP | 2.1 | HDOP | 0.7 | VDOP | 0.9
|  | Base data age | 1 | Positions used | 31 |  |  |  |

Satellites: (GPS) | 3, 4, 8, 9, 16, 26, 28, 31
Satellites: (GLONASS) | 4, 5, 14, 15
Satellites: (GALILEO) | 4, 6, 19, 21, 23, 27, 29
Satellites: (BEIDOU) | 11

QC 2 |  | VCV xx (m²) | 0.000023 | VCV xy (m²) | -0.000001 | VCV xz (m²) | 0.000006 |  |
|  |  |  | VCV yy (m²) | 0.000054 | VCV yz (m²) | -0.000034 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000079 |  |

Feature (1022) | CMON
Depth |
Note | C

Point | 1023 | ΔX | 60696.762 | ΔY | 48354.917 | ΔZ | 45334.156 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.025 | Vt Prec (1 sigma) | 0.033 |  |
QC 1 |  | PDOP | 1.2 | GDOP | 2.1 | HDOP | 0.7 | VDOP | 0.9
|  | Base data age | 1 | Positions used | 34 |  |  |  |

Satellites: (GPS) | 3, 4, 8, 9, 16, 26, 28, 31
Satellites: (GLONASS) | 4, 5, 14, 15
Satellites: (GALILEO) | 4, 6, 19, 21, 23, 27, 29
Satellites: (BEIDOU) | 11

QC 2 |  | VCV xx (m²) | 0.000023 | VCV xy (m²) | -0.000001 | VCV xz (m²) | 0.000007 |  |
|  |  |  | VCV yy (m²) | 0.000055 | VCV yz (m²) | -0.000034 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000078 |  |

Feature (1023) | CMON
Depth |
Note | C

Initialization event: RTK not initialized

GPS week | 2397 | Seconds | 233167 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 233169 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK not initialized

GPS week | 2397 | Seconds | 235171 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 235187 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK not initialized

GPS week | 2397 | Seconds | 235343 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 235359 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK not initialized

GPS week | 2397 | Seconds | 236133 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 236149 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK not initialized

GPS week | 2397 | Seconds | 236242 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 236260 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK not initialized

GPS week | 2397 | Seconds | 236359 | Initialization type | On the fly | Survey type | Real-time |  |

Rover options

Elevation mask | 10 | PDOP mask | 6 |  |  |  |  |  |

Rover options

Elevation mask | 10 | PDOP mask | 6 |  |  |  |  |  |

Survey event

Survey event | Rover started

GNSS receiver

Receiver type | Unknown
Serial number |
Firmware version | 0
Antenna type | AdV Null Antenna
Measurement method | Antenna Phase Center
Tape adjustment | 0.000
Horizontal offset | 0.000
Vertical offset | 0.000

Base point

Point | PRS33667490340 | Antenna height | 0.000 | Type | Corrected |  |  |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 242628 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK not initialized

GPS week | 2397 | Seconds | 242727 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 242729 | Initialization type | On the fly | Survey type | Real-time |  |

GNSS receiver

Receiver type | R12i
Serial number | 6212F02057
Firmware version | 6.14
Antenna type | R12i Internal
Measurement method | Bottom of quick release
Tape adjustment | 0.000
Horizontal offset | 0.000
Vertical offset | 0.588

Point | 1024 | ΔX | 77469.558 | ΔY | 3476.533 | ΔZ | -10020.022 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.040 | Vt Prec (1 sigma) | 0.074 |  |
QC 1 |  | PDOP | 1.6 | GDOP | 2.4 | HDOP | 0.9 | VDOP | 1.4
|  | Base data age | 1 | Positions used | 31 |  |  |  |

Satellites: (GPS) | 2, 4, 7, 8, 9
Satellites: (GLONASS) | 7, 9, 15, 16, 17, 18
Satellites: (GALILEO) | 4, 6, 9, 23, 26, 31

QC 2 |  | VCV xx (m²) | 0.000054 | VCV xy (m²) | 0.000009 | VCV xz (m²) | -0.000016 |  |
|  |  |  | VCV yy (m²) | 0.000402 | VCV yz (m²) | -0.000202 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000200 |  |

Warnings (1024) | Poor precision

Feature (1024) | CMON
Depth |
Note | G

Point | 1025 | ΔX | 77469.476 | ΔY | 3476.342 | ΔZ | -10019.822 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.068 | Vt Prec (1 sigma) | 0.142 |  |
QC 1 |  | PDOP | 1.6 | GDOP | 2.3 | HDOP | 0.8 | VDOP | 1.3
|  | Base data age | 1 | Positions used | 31 |  |  |  |

Satellites: (GPS) | 2, 4, 7, 8, 9
Satellites: (GLONASS) | 7, 9, 15, 16, 17, 18
Satellites: (GALILEO) | 4, 6, 9, 13, 21, 23, 26, 31

QC 2 |  | VCV xx (m²) | 0.000106 | VCV xy (m²) | 0.000010 | VCV xz (m²) | -0.000110 |  |
|  |  |  | VCV yy (m²) | 0.001191 | VCV yz (m²) | -0.000810 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000991 |  |

Warnings (1025) | Poor precision

Feature (1025) | CMON
Depth |
Note | G

Point | 1026 | ΔX | 77469.532 | ΔY | 3476.855 | ΔZ | -10020.183 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.047 | Vt Prec (1 sigma) | 0.104 |  |
QC 1 |  | PDOP | 1.3 | GDOP | 1.9 | HDOP | 0.7 | VDOP | 1.1
|  | Base data age | 1 | Positions used | 30 |  |  |  |

Satellites: (GPS) | 2, 4, 7, 8, 9, 14
Satellites: (GLONASS) | 7, 9, 15, 16, 17, 18
Satellites: (GALILEO) | 4, 6, 9, 21, 23, 26, 31

QC 2 |  | VCV xx (m²) | 0.000075 | VCV xy (m²) | -0.000134 | VCV xz (m²) | 0.000051 |  |
|  |  |  | VCV yy (m²) | 0.000919 | VCV yz (m²) | -0.000363 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000212 |  |

Feature (1026) | CMON
Depth |
Note | G

Point | 1027 | ΔX | 77469.560 | ΔY | 3476.512 | ΔZ | -10020.012 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.033 | Vt Prec (1 sigma) | 0.066 |  |
QC 1 |  | PDOP | 1.5 | GDOP | 2.1 | HDOP | 0.8 | VDOP | 1.2
|  | Base data age | 1 | Positions used | 31 |  |  |  |

Satellites: (GPS) | 2, 4, 7, 8, 9, 14
Satellites: (GLONASS) | 7, 9, 15, 16, 17, 18
Satellites: (GALILEO) | 4, 6, 9, 13, 23, 26, 31

QC 2 |  | VCV xx (m²) | 0.000031 | VCV xy (m²) | -0.000008 | VCV xz (m²) | -0.000003 |  |
|  |  |  | VCV yy (m²) | 0.000359 | VCV yz (m²) | -0.000151 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000110 |  |

Warnings (1027) | Poor precision

Feature (1027) | CMON
Depth |
Note | G

Survey event

Survey event | End survey

Rover options

Elevation mask | 10 | PDOP mask | 6 |  |  |  |  |  |

Rover options

Elevation mask | 10 | PDOP mask | 6 |  |  |  |  |  |

Survey event

Survey event | Rover started

GNSS receiver

Receiver type | Unknown
Serial number |
Firmware version | 0
Antenna type | AdV Null Antenna
Measurement method | Antenna Phase Center
Tape adjustment | 0.000
Horizontal offset | 0.000
Vertical offset | 0.000

Base point

Point | PRS33667490340 | Antenna height | 0.000 | Type | Corrected |  |  |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 310700 | Initialization type | On the fly | Survey type | Real-time |  |

GNSS receiver

Receiver type | R12i
Serial number | 6212F02057
Firmware version | 6.14
Antenna type | R12i Internal
Measurement method | Bottom of quick release
Tape adjustment | 0.000
Horizontal offset | 0.000
Vertical offset | 0.588

Point | 1028 | ΔX | 77469.509 | ΔY | 3476.469 | ΔZ | -10019.982 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.045 | Vt Prec (1 sigma) | 0.071 |  |
QC 1 |  | PDOP | 1.3 | GDOP | 2.3 | HDOP | 0.7 | VDOP | 1.1
|  | Base data age | 1 | Positions used | 31 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 25, 26, 28, 31, 32
Satellites: (GLONASS) | 4, 5, 14, 15
Satellites: (GALILEO) | 2, 3, 7, 8, 13, 26, 30
Satellites: (BEIDOU) | 14

QC 2 |  | VCV xx (m²) | 0.000076 | VCV xy (m²) | 0.000048 | VCV xz (m²) | -0.000009 |  |
|  |  |  | VCV yy (m²) | 0.000405 | VCV yz (m²) | -0.000177 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000179 |  |

Feature (1028) | CMON
Depth |
Note | G

Point | 1029 | ΔX | 77469.495 | ΔY | 3476.370 | ΔZ | -10019.975 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.035 | Vt Prec (1 sigma) | 0.054 |  |
QC 1 |  | PDOP | 1.3 | GDOP | 2.4 | HDOP | 0.7 | VDOP | 1.1
|  | Base data age | 1 | Positions used | 37 |  |  |  |

Satellites: (GPS) | 3, 16, 25, 26, 28, 31, 32
Satellites: (GLONASS) | 4, 5, 14, 15
Satellites: (GALILEO) | 2, 3, 7, 8, 13, 26, 30
Satellites: (BEIDOU) | 14

QC 2 |  | VCV xx (m²) | 0.000049 | VCV xy (m²) | 0.000028 | VCV xz (m²) | -0.000007 |  |
|  |  |  | VCV yy (m²) | 0.000234 | VCV yz (m²) | -0.000105 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000107 |  |

Feature (1029) | CMON
Depth |
Note | G

Point | 1030 | ΔX | 77469.544 | ΔY | 3476.418 | ΔZ | -10020.013 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.037 | Vt Prec (1 sigma) | 0.057 |  |
QC 1 |  | PDOP | 1.5 | GDOP | 2.7 | HDOP | 0.8 | VDOP | 1.3
|  | Base data age | 1 | Positions used | 31 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 25, 26, 28, 31, 32
Satellites: (GLONASS) | 4, 5, 14, 15
Satellites: (GALILEO) | 2, 3, 7, 8, 13, 26, 30
Satellites: (BEIDOU) | 14

QC 2 |  | VCV xx (m²) | 0.000054 | VCV xy (m²) | 0.000023 | VCV xz (m²) | -0.000001 |  |
|  |  |  | VCV yy (m²) | 0.000258 | VCV yz (m²) | -0.000113 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000114 |  |

Feature (1030) | CMON
Depth |
Note | G

Point | 1031 | ΔX | 77469.572 | ΔY | 3476.474 | ΔZ | -10020.022 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.031 | Vt Prec (1 sigma) | 0.047 |  |
QC 1 |  | PDOP | 1.4 | GDOP | 2.5 | HDOP | 0.7 | VDOP | 1.2
|  | Base data age | 1 | Positions used | 31 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 25, 26, 28, 31, 32
Satellites: (GLONASS) | 4, 5, 14, 15
Satellites: (GALILEO) | 2, 3, 7, 8, 13, 25, 26, 30
Satellites: (BEIDOU) | 14

QC 2 |  | VCV xx (m²) | 0.000042 | VCV xy (m²) | 0.000018 | VCV xz (m²) | -0.000003 |  |
|  |  |  | VCV yy (m²) | 0.000169 | VCV yz (m²) | -0.000079 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000087 |  |

Feature (1031) | CMON
Depth |
Note | G

Initialization event: RTK not initialized

GPS week | 2397 | Seconds | 311797 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 311801 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK not initialized

GPS week | 2397 | Seconds | 311849 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 311859 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK not initialized

GPS week | 2397 | Seconds | 312009 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 312026 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK not initialized

GPS week | 2397 | Seconds | 312431 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 312435 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK not initialized

GPS week | 2397 | Seconds | 313019 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 313025 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK not initialized

GPS week | 2397 | Seconds | 313085 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 313090 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK not initialized

GPS week | 2397 | Seconds | 313091 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 313092 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK not initialized

GPS week | 2397 | Seconds | 313272 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 313278 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK not initialized

GPS week | 2397 | Seconds | 313304 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 313318 | Initialization type | On the fly | Survey type | Real-time |  |

Initialization event: RTK not initialized

GPS week | 2397 | Seconds | 313463 | Initialization type | On the fly | Survey type | Real-time |  |

Survey event

Survey event | End survey

Rover options

Elevation mask | 10 | PDOP mask | 6 |  |  |  |  |  |

Rover options

Elevation mask | 10 | PDOP mask | 6 |  |  |  |  |  |

Survey event

Survey event | Rover started

GNSS receiver

Receiver type | Unknown
Serial number |
Firmware version | 0
Antenna type | AdV Null Antenna
Measurement method | Antenna Phase Center
Tape adjustment | 0.000
Horizontal offset | 0.000
Vertical offset | 0.000

Base point

Point | PRS33667490340 | Antenna height | 0.000 | Type | Corrected |  |  |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 313623 | Initialization type | On the fly | Survey type | Real-time |  |

GNSS receiver

Receiver type | R12i
Serial number | 6212F02057
Firmware version | 6.14
Antenna type | R12i Internal
Measurement method | Bottom of quick release
Tape adjustment | 0.000
Horizontal offset | 0.000
Vertical offset | 0.588

Point | 1032 | ΔX | 57114.001 | ΔY | 44865.011 | ΔZ | 42154.557 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.032 | Vt Prec (1 sigma) | 0.052 |  |
QC 1 |  | PDOP | 2.0 | GDOP | 3.2 | HDOP | 0.9 | VDOP | 1.7
|  | Base data age | 1 | Positions used | 39 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 29, 31
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 7, 8, 30

QC 2 |  | VCV xx (m²) | 0.000040 | VCV xy (m²) | 0.000014 | VCV xz (m²) | -0.000018 |  |
|  |  |  | VCV yy (m²) | 0.000162 | VCV yz (m²) | -0.000105 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000142 |  |

Feature (1032) | CMON
Depth |
Note | E

Point | 1033 | ΔX | 57113.981 | ΔY | 44864.894 | ΔZ | 42154.599 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.048 | Vt Prec (1 sigma) | 0.081 |  |
QC 1 |  | PDOP | 2.0 | GDOP | 3.2 | HDOP | 0.9 | VDOP | 1.8
|  | Base data age | 1 | Positions used | 33 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 31
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 7, 8, 30

QC 2 |  | VCV xx (m²) | 0.000087 | VCV xy (m²) | 0.000032 | VCV xz (m²) | -0.000040 |  |
|  |  |  | VCV yy (m²) | 0.000411 | VCV yz (m²) | -0.000254 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000323 |  |

Feature (1033) | CMON
Depth |
Note | E

Point | 1034 | ΔX | 57114.058 | ΔY | 44865.051 | ΔZ | 42154.569 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.039 | Vt Prec (1 sigma) | 0.069 |  |
QC 1 |  | PDOP | 2.0 | GDOP | 3.2 | HDOP | 0.9 | VDOP | 1.8
|  | Base data age | 1 | Positions used | 31 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 29, 31, 32
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 7, 8, 25, 30

QC 2 |  | VCV xx (m²) | 0.000059 | VCV xy (m²) | 0.000053 | VCV xz (m²) | -0.000042 |  |
|  |  |  | VCV yy (m²) | 0.000321 | VCV yz (m²) | -0.000196 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000210 |  |

Feature (1034) | CMON
Depth |
Note | E

Point | 1035 | ΔX | 57113.964 | ΔY | 44864.931 | ΔZ | 42154.677 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.044 | Vt Prec (1 sigma) | 0.075 |  |
QC 1 |  | PDOP | 2.0 | GDOP | 3.2 | HDOP | 0.9 | VDOP | 1.8
|  | Base data age | 1 | Positions used | 33 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 29, 31
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 7, 8, 30

QC 2 |  | VCV xx (m²) | 0.000068 | VCV xy (m²) | 0.000024 | VCV xz (m²) | -0.000029 |  |
|  |  |  | VCV yy (m²) | 0.000343 | VCV yz (m²) | -0.000220 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000290 |  |

Feature (1035) | CMON
Depth |
Note | E

Point | 1036 | ΔX | 57071.687 | ΔY | 44866.316 | ΔZ | 42164.458 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.037 | Vt Prec (1 sigma) | 0.064 |  |
QC 1 |  | PDOP | 1.4 | GDOP | 2.6 | HDOP | 0.8 | VDOP | 1.2
|  | Base data age | 1 | Positions used | 33 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 29, 31, 32
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 7, 8, 25, 30
Satellites: (BEIDOU) | 14

QC 2 |  | VCV xx (m²) | 0.000046 | VCV xy (m²) | -0.000001 | VCV xz (m²) | -0.000007 |  |
|  |  |  | VCV yy (m²) | 0.000244 | VCV yz (m²) | -0.000156 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000218 |  |

Feature (1036) | CMON
Depth |
Note | D

Point | 1037 | ΔX | 57071.672 | ΔY | 44866.291 | ΔZ | 42164.540 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.031 | Vt Prec (1 sigma) | 0.050 |  |
QC 1 |  | PDOP | 1.3 | GDOP | 2.4 | HDOP | 0.8 | VDOP | 1.1
|  | Base data age | 1 | Positions used | 31 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 29, 31, 32
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 3, 7, 8, 25, 30
Satellites: (BEIDOU) | 14

QC 2 |  | VCV xx (m²) | 0.000034 | VCV xy (m²) | -0.000008 | VCV xz (m²) | 0.000002 |  |
|  |  |  | VCV yy (m²) | 0.000156 | VCV yz (m²) | -0.000090 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000134 |  |

Feature (1037) | CMON
Depth |
Note | D

Point | 1038 | ΔX | 57071.640 | ΔY | 44866.249 | ΔZ | 42164.534 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.028 | Vt Prec (1 sigma) | 0.046 |  |
QC 1 |  | PDOP | 1.3 | GDOP | 2.4 | HDOP | 0.8 | VDOP | 1.1
|  | Base data age | 1 | Positions used | 33 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 29, 31
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 7, 8, 25, 30

QC 2 |  | VCV xx (m²) | 0.000028 | VCV xy (m²) | -0.000005 | VCV xz (m²) | -0.000002 |  |
|  |  |  | VCV yy (m²) | 0.000137 | VCV yz (m²) | -0.000075 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000102 |  |

Feature (1038) | CMON
Depth |
Note | D

Point | 1039 | ΔX | 57071.689 | ΔY | 44866.254 | ΔZ | 42164.506 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.029 | Vt Prec (1 sigma) | 0.052 |  |
QC 1 |  | PDOP | 2.0 | GDOP | 3.2 | HDOP | 0.9 | VDOP | 1.8
|  | Base data age | 1 | Positions used | 33 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 29, 31
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 7, 8, 25, 30

QC 2 |  | VCV xx (m²) | 0.000032 | VCV xy (m²) | -0.000000 | VCV xz (m²) | -0.000002 |  |
|  |  |  | VCV yy (m²) | 0.000166 | VCV yz (m²) | -0.000102 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000130 |  |

Feature (1039) | CMON
Depth |
Note | D

Point | 1040 | ΔX | 57094.533 | ΔY | 45088.302 | ΔZ | 42399.364 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.026 | Vt Prec (1 sigma) | 0.042 |  |
QC 1 |  | PDOP | 1.6 | GDOP | 2.9 | HDOP | 0.8 | VDOP | 1.4
|  | Base data age | 1 | Positions used | 41 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 31, 32
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 3, 7, 8, 30

QC 2 |  | VCV xx (m²) | 0.000027 | VCV xy (m²) | -0.000007 | VCV xz (m²) | 0.000003 |  |
|  |  |  | VCV yy (m²) | 0.000112 | VCV yz (m²) | -0.000063 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000084 |  |

Feature (1040) | CMON
Depth |
Note | F

Point | 1041 | ΔX | 57094.559 | ΔY | 45088.252 | ΔZ | 42399.375 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.030 | Vt Prec (1 sigma) | 0.051 |  |
QC 1 |  | PDOP | 1.6 | GDOP | 2.6 | HDOP | 0.8 | VDOP | 1.4
|  | Base data age | 1 | Positions used | 31 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 31, 32
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 3, 7, 8, 30

QC 2 |  | VCV xx (m²) | 0.000035 | VCV xy (m²) | -0.000004 | VCV xz (m²) | -0.000001 |  |
|  |  |  | VCV yy (m²) | 0.000162 | VCV yz (m²) | -0.000100 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000130 |  |

Feature (1041) | CMON
Depth |
Note | F

Point | 1042 | ΔX | 57094.594 | ΔY | 45088.319 | ΔZ | 42399.393 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.030 | Vt Prec (1 sigma) | 0.051 |  |
QC 1 |  | PDOP | 1.5 | GDOP | 2.3 | HDOP | 0.8 | VDOP | 1.2
|  | Base data age | 1 | Positions used | 34 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 31, 32
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 3, 7, 8, 30

QC 2 |  | VCV xx (m²) | 0.000037 | VCV xy (m²) | -0.000008 | VCV xz (m²) | 0.000001 |  |
|  |  |  | VCV yy (m²) | 0.000164 | VCV yz (m²) | -0.000097 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000125 |  |

Feature (1042) | CMON
Depth |
Note | F

Point | 1043 | ΔX | 57094.549 | ΔY | 45088.307 | ΔZ | 42399.429 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.028 | Vt Prec (1 sigma) | 0.046 |  |
QC 1 |  | PDOP | 1.6 | GDOP | 2.5 | HDOP | 0.8 | VDOP | 1.3
|  | Base data age | 1 | Positions used | 33 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 31, 32
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 3, 7, 8, 30

QC 2 |  | VCV xx (m²) | 0.000032 | VCV xy (m²) | -0.000009 | VCV xz (m²) | 0.000004 |  |
|  |  |  | VCV yy (m²) | 0.000136 | VCV yz (m²) | -0.000077 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000101 |  |

Feature (1043) | CMON
Depth |
Note | F

Initialization event: RTK not initialized

GPS week | 2397 | Seconds | 314787 | Initialization type | On the fly | Survey type | Real-time |  |

Survey event

Survey event | End survey

Rover options

Elevation mask | 10 | PDOP mask | 6 |  |  |  |  |  |

Rover options

Elevation mask | 10 | PDOP mask | 6 |  |  |  |  |  |

Survey event

Survey event | Rover started

Point | PRS87952758624 | Latitude | 40°24'16.24600"N | Longitude | 80°43'17.24702"W | Height | 1109.615 | Code |

GNSS receiver

Receiver type | Unknown
Serial number |
Firmware version | 0
Antenna type | AdV Null Antenna
Measurement method | Antenna Phase Center
Tape adjustment | 0.000
Horizontal offset | 0.000
Vertical offset | 0.000

Base point

Point | PRS87952758624 | Antenna height | 0.000 | Type | Corrected |  |  |  |

Initialization event: RTK initialized

GPS week | 2397 | Seconds | 315329 | Initialization type | On the fly | Survey type | Real-time |  |

GNSS receiver

Receiver type | R12i
Serial number | 6212F02057
Firmware version | 6.14
Antenna type | R12i Internal
Measurement method | Bottom of quick release
Tape adjustment | 0.000
Horizontal offset | 0.000
Vertical offset | 0.588

Point | 1044 | ΔX | -79103.701 | ΔY | -21967.787 | ΔZ | -11043.142 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.024 | Vt Prec (1 sigma) | 0.037 |  |
QC 1 |  | PDOP | 1.1 | GDOP | 1.9 | HDOP | 0.7 | VDOP | 0.9
|  | Base data age | 1 | Positions used | 36 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 29, 31
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 7, 8, 27, 30
Satellites: (BEIDOU) | 23, 24, 25, 32, 33, 41

QC 2 |  | VCV xx (m²) | 0.000026 | VCV xy (m²) | -0.000011 | VCV xz (m²) | 0.000002 |  |
|  |  |  | VCV yy (m²) | 0.000087 | VCV yz (m²) | -0.000046 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000067 |  |

Feature (1044) | CMON
Depth |
Note | A

Point | 1045 | ΔX | -79103.678 | ΔY | -21967.761 | ΔZ | -11043.115 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.022 | Vt Prec (1 sigma) | 0.034 |  |
QC 1 |  | PDOP | 1.1 | GDOP | 1.9 | HDOP | 0.7 | VDOP | 0.9
|  | Base data age | 1 | Positions used | 35 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 29, 31
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 7, 8, 27, 30
Satellites: (BEIDOU) | 23, 24, 25, 32, 33, 41

QC 2 |  | VCV xx (m²) | 0.000022 | VCV xy (m²) | -0.000010 | VCV xz (m²) | 0.000003 |  |
|  |  |  | VCV yy (m²) | 0.000075 | VCV yz (m²) | -0.000041 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000058 |  |

Feature (1045) | CMON
Depth |
Note | A

Point | 1046 | ΔX | -79103.707 | ΔY | -21967.764 | ΔZ | -11043.101 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.021 | Vt Prec (1 sigma) | 0.033 |  |
QC 1 |  | PDOP | 1.2 | GDOP | 2.0 | HDOP | 0.7 | VDOP | 0.9
|  | Base data age | 1 | Positions used | 37 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 29, 31
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 7, 8, 27, 30
Satellites: (BEIDOU) | 23, 24, 25, 32, 33, 41

QC 2 |  | VCV xx (m²) | 0.000020 | VCV xy (m²) | -0.000009 | VCV xz (m²) | 0.000002 |  |
|  |  |  | VCV yy (m²) | 0.000068 | VCV yz (m²) | -0.000037 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000052 |  |

Feature (1046) | CMON
Depth |
Note | A

Point | 1047 | ΔX | -79103.703 | ΔY | -21967.778 | ΔZ | -11043.116 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.020 | Vt Prec (1 sigma) | 0.032 |  |
QC 1 |  | PDOP | 1.2 | GDOP | 2.0 | HDOP | 0.7 | VDOP | 0.9
|  | Base data age | 1 | Positions used | 31 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 29, 31
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 7, 8, 27, 30
Satellites: (BEIDOU) | 23, 24, 25, 32, 33, 41

QC 2 |  | VCV xx (m²) | 0.000018 | VCV xy (m²) | -0.000008 | VCV xz (m²) | 0.000002 |  |
|  |  |  | VCV yy (m²) | 0.000064 | VCV yz (m²) | -0.000035 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000048 |  |

Feature (1047) | CMON
Depth |
Note | A

Point | 1048 | ΔX | -79324.075 | ΔY | -22080.782 | ΔZ | -11144.453 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.022 | Vt Prec (1 sigma) | 0.033 |  |
QC 1 |  | PDOP | 1.1 | GDOP | 1.8 | HDOP | 0.7 | VDOP | 0.9
|  | Base data age | 1 | Positions used | 31 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 29, 31
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 3, 7, 8, 27, 30
Satellites: (BEIDOU) | 23, 24, 25, 32, 33, 41

QC 2 |  | VCV xx (m²) | 0.000023 | VCV xy (m²) | -0.000014 | VCV xz (m²) | 0.000006 |  |
|  |  |  | VCV yy (m²) | 0.000069 | VCV yz (m²) | -0.000038 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000056 |  |

Feature (1048) | CMON
Depth |
Note | B

Point | 1049 | ΔX | -79324.070 | ΔY | -22080.821 | ΔZ | -11144.458 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.020 | Vt Prec (1 sigma) | 0.031 |  |
QC 1 |  | PDOP | 1.1 | GDOP | 1.8 | HDOP | 0.7 | VDOP | 0.9
|  | Base data age | 1 | Positions used | 38 |  |  |  |

Satellites: (GPS) | 3, 4, 16, 26, 28, 29, 31
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 3, 7, 8, 27, 30
Satellites: (BEIDOU) | 23, 24, 25, 32, 33, 41

QC 2 |  | VCV xx (m²) | 0.000020 | VCV xy (m²) | -0.000012 | VCV xz (m²) | 0.000005 |  |
|  |  |  | VCV yy (m²) | 0.000061 | VCV yz (m²) | -0.000034 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000049 |  |

Feature (1049) | CMON
Depth |
Note | B

Point | 1050 | ΔX | -79324.023 | ΔY | -22080.826 | ΔZ | -11144.460 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.019 | Vt Prec (1 sigma) | 0.030 |  |
QC 1 |  | PDOP | 1.2 | GDOP | 2.0 | HDOP | 0.7 | VDOP | 0.9
|  | Base data age | 1 | Positions used | 30 |  |  |  |

Satellites: (GPS) | 3, 4, 9, 16, 26, 28, 29, 31
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 7, 8, 27, 30
Satellites: (BEIDOU) | 23, 24, 25, 32, 33, 41

QC 2 |  | VCV xx (m²) | 0.000018 | VCV xy (m²) | -0.000011 | VCV xz (m²) | 0.000004 |  |
|  |  |  | VCV yy (m²) | 0.000055 | VCV yz (m²) | -0.000031 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000044 |  |

Feature (1050) | CMON
Depth |
Note | B

Point | 1051 | ΔX | -79324.023 | ΔY | -22080.809 | ΔZ | -11144.452 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.018 | Vt Prec (1 sigma) | 0.029 |  |
QC 1 |  | PDOP | 1.2 | GDOP | 2.0 | HDOP | 0.7 | VDOP | 0.9
|  | Base data age | 1 | Positions used | 32 |  |  |  |

Satellites: (GPS) | 3, 4, 9, 16, 26, 28, 29, 31
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 7, 8, 27, 30
Satellites: (BEIDOU) | 23, 24, 25, 32, 33, 41

QC 2 |  | VCV xx (m²) | 0.000016 | VCV xy (m²) | -0.000009 | VCV xz (m²) | 0.000004 |  |
|  |  |  | VCV yy (m²) | 0.000053 | VCV yz (m²) | -0.000031 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000042 |  |

Feature (1051) | CMON
Depth |
Note | B

Point | 1052 | ΔX | -79609.451 | ΔY | -22132.855 | ΔZ | -11162.714 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.020 | Vt Prec (1 sigma) | 0.031 |  |
QC 1 |  | PDOP | 1.0 | GDOP | 1.7 | HDOP | 0.6 | VDOP | 0.8
|  | Base data age | 1 | Positions used | 33 |  |  |  |

Satellites: (GPS) | 3, 4, 9, 16, 26, 28, 29, 31
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 7, 8, 27, 29, 30
Satellites: (BEIDOU) | 23, 24, 25, 32, 33, 41

QC 2 |  | VCV xx (m²) | 0.000018 | VCV xy (m²) | -0.000011 | VCV xz (m²) | 0.000004 |  |
|  |  |  | VCV yy (m²) | 0.000060 | VCV yz (m²) | -0.000034 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000046 |  |

Feature (1052) | CMON
Depth |
Note | C

Point | 1053 | ΔX | -79609.475 | ΔY | -22132.848 | ΔZ | -11162.728 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.019 | Vt Prec (1 sigma) | 0.030 |  |
QC 1 |  | PDOP | 1.0 | GDOP | 1.7 | HDOP | 0.6 | VDOP | 0.8
|  | Base data age | 1 | Positions used | 32 |  |  |  |

Satellites: (GPS) | 3, 4, 9, 16, 26, 28, 29, 31
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 7, 8, 27, 29, 30
Satellites: (BEIDOU) | 23, 24, 25, 32, 33, 41

QC 2 |  | VCV xx (m²) | 0.000017 | VCV xy (m²) | -0.000009 | VCV xz (m²) | 0.000004 |  |
|  |  |  | VCV yy (m²) | 0.000058 | VCV yz (m²) | -0.000032 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000042 |  |

Feature (1053) | CMON
Depth |
Note | C

Point | 1054 | ΔX | -79609.473 | ΔY | -22132.856 | ΔZ | -11162.753 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.018 | Vt Prec (1 sigma) | 0.030 |  |
QC 1 |  | PDOP | 1.0 | GDOP | 1.8 | HDOP | 0.6 | VDOP | 0.8
|  | Base data age | 1 | Positions used | 35 |  |  |  |

Satellites: (GPS) | 3, 4, 9, 16, 26, 28, 29, 31
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 7, 8, 27, 29, 30
Satellites: (BEIDOU) | 23, 24, 25, 32, 33, 41

QC 2 |  | VCV xx (m²) | 0.000016 | VCV xy (m²) | -0.000008 | VCV xz (m²) | 0.000003 |  |
|  |  |  | VCV yy (m²) | 0.000058 | VCV yz (m²) | -0.000032 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000040 |  |

Feature (1054) | CMON
Depth |
Note | C

Point | 1055 | ΔX | -79609.459 | ΔY | -22132.840 | ΔZ | -11162.751 | Code | CMON
|  | Method | Network RTK | Type | Observed control point | Search class | Normal |  |
Antenna height | 6.562 | Type | Uncorrected | Hz Prec (DRMS) | 0.018 | Vt Prec (1 sigma) | 0.029 |  |
QC 1 |  | PDOP | 1.0 | GDOP | 1.7 | HDOP | 0.6 | VDOP | 0.8
|  | Base data age | 1 | Positions used | 30 |  |  |  |

Satellites: (GPS) | 3, 4, 9, 16, 26, 28, 29, 31
Satellites: (GLONASS) | 4, 5, 14, 15, 16
Satellites: (GALILEO) | 2, 7, 8, 27, 29, 30
Satellites: (BEIDOU) | 23, 24, 25, 32, 33, 41

QC 2 |  | VCV xx (m²) | 0.000015 | VCV xy (m²) | -0.000008 | VCV xz (m²) | 0.000002 |  |
|  |  |  | VCV yy (m²) | 0.000056 | VCV yz (m²) | -0.000030 |  |
|  |  |  |  |  | VCV zz (m²) | 0.000038 |  |

Feature (1055) | CMON
Depth |
Note | C

Note | Exported file: /storage/emulated/0/Trimble Data/Projects/ODOT D11 culverts/ODOT D11 culverts.csv

Note | Exported file: /storage/emulated/0/Trimble Data/Projects/ODOT D11 culverts/ODOT D11 culverts.jxl

Reduced points

Point | 5001 | North | 258014.023 | East | 2382495.544 | Elevation | 1016.207 | Code | CNPT-A

Point | 5002 | North | 257882.826 | East | 2382262.423 | Elevation | 1009.484 | Code | CNPT-B

Point | 5003 | North | 257882.862 | East | 2382262.434 | Elevation | 1009.490 | Code | CNPT-B

Point | 5004 | North | 257882.850 | East | 2382262.410 | Elevation | 1009.513 | Code | CNPT-B

Point | 5005 | North | 257882.855 | East | 2382262.411 | Elevation | 1009.496 | Code | CNPT-B

Point | 5006 | North | 257859.556 | East | 2381972.793 | Elevation | 1002.834 | Code | CNPT-C

Point | 5007 | North | 257859.560 | East | 2381972.768 | Elevation | 1002.842 | Code | CNPT-C

Point | 5008 | North | 257859.607 | East | 2381972.782 | Elevation | 1002.819 | Code | CNPT-C

Point | 5009 | North | 257859.609 | East | 2381972.762 | Elevation | 1002.810 | Code | CNPT-C

Point | 5010 | North | 258014.060 | East | 2382495.589 | Elevation | 1016.251 | Code | CNPT-A

Point | 5011 | North | 258014.082 | East | 2382495.597 | Elevation | 1016.243 | Code | CNPT-A

Point | 5012 | North | 258014.079 | East | 2382495.569 | Elevation | 1016.238 | Code | CNPT-A

Point | 5013 | North | 253509.984 | East | 2377920.883 | Elevation | 1144.999 | Code | CNPT-D

Point | 5014 | North | 253509.975 | East | 2377920.939 | Elevation | 1144.992 | Code | CNPT-D

Point | 5015 | North | 253509.973 | East | 2377920.917 | Elevation | 1145.082 | Code | CNPT-D

Point | 5016 | North | 253509.968 | East | 2377920.885 | Elevation | 1145.123 | Code | CNPT-D

Point | 5017 | North | 253498.000 | East | 2377962.746 | Elevation | 1144.597 | Code | CNPT-E

Point | 5018 | North | 253498.024 | East | 2377962.721 | Elevation | 1144.595 | Code | CNPT-E

Point | 5019 | North | 253498.016 | East | 2377962.777 | Elevation | 1144.534 | Code | CNPT-E

Point | 5020 | North | 253498.010 | East | 2377962.754 | Elevation | 1144.605 | Code | CNPT-E

Point | 5021 | North | 253829.595 | East | 2377972.687 | Elevation | 1132.795 | Code | CNPT-F

Point | 5022 | North | 253829.601 | East | 2377972.662 | Elevation | 1132.800 | Code | CNPT-F

Point | 5023 | North | 253829.572 | East | 2377972.700 | Elevation | 1132.834 | Code | CNPT-F

Point | 5024 | North | 253829.608 | East | 2377972.708 | Elevation | 1132.781 | Code | CNPT-F

Point | 5025 | North | 185451.446 | East | 2392765.419 | Elevation | 1051.787 | Code | CNPT-G

Point | 5026 | North | 185451.461 | East | 2392765.426 | Elevation | 1051.786 | Code | CNPT-G

Point | 5027 | North | 185451.455 | East | 2392765.430 | Elevation | 1051.765 | Code | CNPT-G

Point | 5028 | North | 185451.471 | East | 2392765.399 | Elevation | 1051.753 | Code | CNPT-G

Point | PRS33667490340 | North | 197385.417 | East | 2315488.116 | Elevation | 1011.841 | Code |

Point | 1000 | North | 253498.030 | East | 2377962.688 | Elevation | 1144.636 | Code | CMON

Point | 1001 | North | 253498.023 | East | 2377962.696 | Elevation | 1144.746 | Code | CMON

Point | 1002 | North | 253498.017 | East | 2377962.778 | Elevation | 1144.662 | Code | CMON

Point | 1003 | North | 253498.040 | East | 2377962.765 | Elevation | 1144.633 | Code | CMON

Point | 1004 | North | 253509.973 | East | 2377920.898 | Elevation | 1145.015 | Code | CMON

Point | 1005 | North | 253510.011 | East | 2377920.859 | Elevation | 1145.012 | Code | CMON

Point | 1006 | North | 253510.017 | East | 2377920.788 | Elevation | 1145.041 | Code | CMON

Point | 1007 | North | 253509.982 | East | 2377920.789 | Elevation | 1145.000 | Code | CMON

Point | 1008 | North | 253829.575 | East | 2377972.630 | Elevation | 1132.849 | Code | CMON

Point | 1009 | North | 253829.564 | East | 2377972.705 | Elevation | 1132.829 | Code | CMON

Point | 1010 | North | 253829.578 | East | 2377972.763 | Elevation | 1132.750 | Code | CMON

Point | 1011 | North | 253829.563 | East | 2377972.705 | Elevation | 1132.777 | Code | CMON

Point | 1012 | North | 258014.047 | East | 2382495.524 | Elevation | 1016.338 | Code | CMON

Point | 1013 | North | 258014.083 | East | 2382495.539 | Elevation | 1016.340 | Code | CMON

Point | 1014 | North | 258014.088 | East | 2382495.506 | Elevation | 1016.303 | Code | CMON

Point | 1015 | North | 258014.067 | East | 2382495.473 | Elevation | 1016.316 | Code | CMON

Point | 1016 | North | 257882.841 | East | 2382262.357 | Elevation | 1009.494 | Code | CMON

Point | 1017 | North | 257882.821 | East | 2382262.353 | Elevation | 1009.482 | Code | CMON

Point | 1018 | North | 257882.809 | East | 2382262.371 | Elevation | 1009.451 | Code | CMON

Point | 1019 | North | 257882.831 | East | 2382262.388 | Elevation | 1009.445 | Code | CMON

Point | 1020 | North | 257859.563 | East | 2381972.715 | Elevation | 1002.868 | Code | CMON

Point | 1021 | North | 257859.542 | East | 2381972.687 | Elevation | 1002.867 | Code | CMON

Point | 1022 | North | 257859.526 | East | 2381972.698 | Elevation | 1002.864 | Code | CMON

Point | 1023 | North | 257859.543 | East | 2381972.719 | Elevation | 1002.883 | Code | CMON

Point | 1024 | North | 185451.491 | East | 2392765.317 | Elevation | 1051.737 | Code | CMON

Point | 1025 | North | 185451.529 | East | 2392765.206 | Elevation | 1052.000 | Code | CMON

Point | 1026 | North | 185451.577 | East | 2392765.340 | Elevation | 1051.386 | Code | CMON

Point | 1027 | North | 185451.485 | East | 2392765.316 | Elevation | 1051.759 | Code | CMON

Point | 1028 | North | 185451.485 | East | 2392765.259 | Elevation | 1051.805 | Code | CMON

Point | 1029 | North | 185451.428 | East | 2392765.230 | Elevation | 1051.882 | Code | CMON

Point | 1030 | North | 185451.426 | East | 2392765.287 | Elevation | 1051.828 | Code | CMON

Point | 1031 | North | 185451.452 | East | 2392765.322 | Elevation | 1051.783 | Code | CMON

Point | 1032 | North | 253498.017 | East | 2377962.698 | Elevation | 1144.600 | Code | CMON

Point | 1033 | North | 253497.975 | East | 2377962.661 | Elevation | 1144.712 | Code | CMON

Point | 1034 | North | 253498.047 | East | 2377962.760 | Elevation | 1144.584 | Code | CMON

Point | 1035 | North | 253498.060 | East | 2377962.648 | Elevation | 1144.732 | Code | CMON

Point | 1036 | North | 253509.965 | East | 2377920.899 | Elevation | 1145.000 | Code | CMON

Point | 1037 | North | 253510.013 | East | 2377920.880 | Elevation | 1145.071 | Code | CMON

Point | 1038 | North | 253509.984 | East | 2377920.842 | Elevation | 1145.094 | Code | CMON

Point | 1039 | North | 253509.962 | East | 2377920.892 | Elevation | 1145.079 | Code | CMON

Point | 1040 | North | 253829.558 | East | 2377972.696 | Elevation | 1132.717 | Code | CMON

Point | 1041 | North | 253829.532 | East | 2377972.714 | Elevation | 1132.765 | Code | CMON

Point | 1042 | North | 253829.586 | East | 2377972.759 | Elevation | 1132.730 | Code | CMON

Point | 1043 | North | 253829.610 | East | 2377972.712 | Elevation | 1132.758 | Code | CMON

Point | PRS87952758624 | North | 273867.841 | East | 2463797.592 | Elevation | 1221.282 | Code |

Point | 1044 | North | 258014.049 | East | 2382495.516 | Elevation | 1016.256 | Code | CMON

Point | 1045 | North | 258014.084 | East | 2382495.541 | Elevation | 1016.256 | Code | CMON

Point | 1046 | North | 258014.096 | East | 2382495.512 | Elevation | 1016.264 | Code | CMON

Point | 1047 | North | 258014.075 | East | 2382495.514 | Elevation | 1016.265 | Code | CMON

Point | 1048 | North | 257882.879 | East | 2382262.405 | Elevation | 1009.453 | Code | CMON

Point | 1049 | North | 257882.850 | East | 2382262.404 | Elevation | 1009.480 | Code | CMON

Point | 1050 | North | 257882.841 | East | 2382262.450 | Elevation | 1009.487 | Code | CMON

Point | 1051 | North | 257882.858 | East | 2382262.453 | Elevation | 1009.481 | Code | CMON

Point | 1052 | North | 257859.585 | East | 2381972.761 | Elevation | 1002.857 | Code | CMON

Point | 1053 | North | 257859.581 | East | 2381972.739 | Elevation | 1002.840 | Code | CMON

Point | 1054 | North | 257859.557 | East | 2381972.740 | Elevation | 1002.830 | Code | CMON

Point | 1055 | North | 257859.567 | East | 2381972.756 | Elevation | 1002.821 | Code | CMON