**PID 105777 Existing Documents**

PID 105777 LAK-2-11.41 Deck Hendricks over SR - 2

The bridge was constructed around 1960. The bridge was painted in 1999. In 2001 the bridge received a new wearing surface. In 2017 the spalls were removed, and the bridge was sub decked.

Past construction plans can be obtained from the District 12 map room located at the district 12 office. A sampling of the following plans are located on the ODOT FTP site:

**ftp://ftp.dot.state.oh.us/pub/Districts/D12/Production/Consultant\_Programmatic/105777/**

**C/R/S Year Directory Pages**

**LAK-2-10.35, YR 1960 SD 000918 1, 319-324**

**CUY-2-0.55, YR 1999 SD 000907 1-15**

**CUY-2-11.4, YR 2001 SD 000919 1-9**

**D-12 BH 99, YR 2017 SD 003336 1-42**

Past Bridge inspections and current bridge inventory can be found at: http://biareports.dot.state.oh.us/