**Pavement Repair QTY Estimates for SR128 5.64 – 5.89 (HAM114855)**

* MM5.64 – 5.70
  + Pavement condition is decent, but some rutting on NB lanes closer to intersection
  + 4’ x 1o0’ = 400 SF = **44 SY**
* MM5.70 – 5.83
  + Some transverse and longitudinal cracking throughout; severe rutting closer to intersection on SB lanes & minimal rutting throughout other areas
  + ~1770 SF = **200 SY**
* For a total of ~250 SY. Not sure when work will begin, but perhaps attaching a 10% value would account for future deterioration.
* An estimated range for pavement repairs would be **275 - 325 SY**.
* MM5.83 – 5.89
  + Pavement Repairs don’t look to be needed – pavement condition was fair