{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Estimated Quantities"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Estimated Quantities","index":0,"n_rows":40,"n_cols":14,"rows_kept":40,"cut":false,"hidden":false,"merged":[[12,9,12,12],[9,9,9,12],[36,9,36,12],[17,9,17,12],[18,9,18,12],[19,9,19,12],[22,9,22,12],[24,9,24,12],[23,9,23,12],[20,9,20,12],[14,9,14,12],[15,9,15,12],[16,9,16,12],[26,9,26,12],[25,9,25,12],[27,9,27,12],[2,12,2,13],[3,12,3,13],[2,10,2,11],[3,10,3,11],[2,2,3,9],[4,9,4,12],[7,9,7,12],[8,9,8,12],[10,9,10,12],[11,9,11,12],[39,9,39,12],[35,9,35,12],[33,9,33,12],[34,9,34,12],[37,9,37,12]]}
[]
[]
[null,null,"ESTIMATED QUANTITIES",null,null,null,null,null,null,null,"DESIGNED:ERK",null,"CHECKED:GDJ"]
[null,null,null,null,null,null,null,null,null,null,"DATE: 11/1/2018",null,"DATE:11/1/2018"]
[null,null,"ITEM","EXTENSION","WALL 1","WALL 2","WALL 3","TOTAL","UNIT","DESCRIPTION",null,null,null,"SHEET #"]
[null,null,203,35150,null,null,15,{"$f":"SUM(E6:G6)","v":15},"CY","GRANULAR MATERIAL, TYPE F"]
[]
[null,null,503,21300,"LS","LS",null,"LS","-","UNCLASSIFIED EXCAVATION"]
[]
[null,null,507,400,null,null,1895,{"$f":"SUM(E10:G10)","v":1895},"FT","STEEL PILES, MISC.:  SOLDIER PILES HP14X73",null,null,null,"84"]
[null,null,507,400,876,null,null,{"$f":"SUM(E11:G11)","v":876},"FT","STEEL PILES, MISC.:  SOLDIER PILES HP14X89",null,null,null,"84"]
[null,null,507,400,1578,null,null,{"$f":"SUM(E12:G12)","v":1578},"FT","STEEL PILES, MISC.:  SOLDIER PILES HP14X117",null,null,null,"84"]
[null,null,507,400,null,3267,null,{"$f":"SUM(E13:G13)","v":3267},"FT","STEEL PILES, MISC.:  SOLDIER PILES W27X84",null,null,null,"84"]
[]
[null,null,509,10000,12638,19802,null,{"$f":"SUM(E15:G15)","v":32440},"LB","EPOXY COATED REINFORCING STEEL"]
[]
[null,null,511,46010,197,209,null,{"$f":"SUM(E17:G17)","v":406},"CY","CLASS QC1 CONCRETE, RETAINING/WINGWALL NOT INCLUDING FOOTING"]
[null,null,511,81300,63,null,null,{"$f":"SUM(E18:G18)","v":63},"EACH","CONCRETE, MISC.: 8\" X 24\" X 69\" PRECAST CONCRETE LAGGING",null,null,null,"84"]
[null,null,511,81300,69,null,null,{"$f":"SUM(E19:G19)","v":69},"EACH","CONCRETE, MISC.: 8\" X 36\" X 69\" PRECAST CONCRETE LAGGING",null,null,null,"84"]
[null,null,511,81300,30,null,null,{"$f":"SUM(E20:G20)","v":30},"EACH","CONCRETE, MISC.: 8\" X 24\" X 69\" PRECAST CONCRETE LAGGING WITH OPENING",null,null,null,"84"]
[null,null,511,81300,30,null,null,{"$f":"SUM(E21:G21)","v":30},"EACH","CONCRETE, MISC.: 8\" X 36\" X 69\" PRECAST CONCRETE LAGGING WITH OPENING",null,null,null,"84"]
[]
[null,null,511,81300,null,null,41,{"$f":"SUM(E23:G23)","v":41},"EACH","CONCRETE, MISC.: 8\" X 24\" X 93\" PRECAST CONCRETE LAGGING",null,null,null,"84"]
[null,null,511,81300,null,null,94,{"$f":"SUM(E24:G24)","v":94},"EACH","CONCRETE, MISC.: 8\" X 36\" X 93\" PRECAST CONCRETE LAGGING",null,null,null,"84"]
[null,null,511,81300,null,null,47,{"$f":"SUM(E25:G25)","v":47},"EACH","CONCRETE, MISC.: 8\" X 24\" X 93\" PRECAST CONCRETE LAGGING WITH OPENING",null,null,null,"84"]
[]
[null,null,512,10100,469,490,null,{"$f":"SUM(E27:G27)","v":959},"SY","SEALING OF CONCRETE SURFACES (EPOXY-URETHANE)"]
[null,null,512,33000,7,9,null,{"$f":"SUM(E28:G28)","v":16},"SY","TYPE 2 WATERPROOFING"]
[]
[null,null,516,13600,58,60,null,{"$f":"SUM(E30:G30)","v":118},"SF","1\" PREFORMED EXPANSION JOINT FILLER"]
[]
[null,null,517,70000,658,863,null,{"$f":"SUM(E32:G32)","v":1521},"FT","RAILING (TWIN STEEL TUBE)"]
[]
[null,null,524,94603,300,null,null,{"$f":"SUM(E34:G34)","v":300},"FT","DRILLED SHAFTS, 30\" DIAMETER, ABOVE BEDROCK, AS PER PLAN",null,null,null,"84"]
[null,null,524,94605,420,null,null,{"$f":"SUM(E35:G35)","v":420},"FT","DRILLED SHAFTS, 30\" DIAMETER, INTO BEDROCK, AS PER PLAN",null,null,null,"84"]
[null,null,524,94703,1830,2150,1348,{"$f":"SUM(E36:G36)","v":5328},"FT","DRILLED SHAFTS, 36\" DIAMETER, ABOVE BEDROCK, AS PER PLAN",null,null,null,"84"]
[null,null,524,94705,1728,1440,500,{"$f":"SUM(E37:G37)","v":3668},"FT","DRILLED SHAFTS, 36\" DIAMETER, INTO BEDROCK, AS PER PLAN",null,null,null,"84"]
[null,null,524,95000,1378,1420,null,{"$f":"SUM(E38:G38)","v":2798},"FT","DRILLED SHAFTS, MISC.: PLUG SHAFT, 42\" DIAMETER, UNREINFORCED",null,null,null,"84"]
[]
[null,null,"SPECIAL",53000600,1049,null,2488,{"$f":"SUM(E40:G40)","v":3537},"SF","STRUCTURES:  PREFABRICATED GEOCOMPOSITE DRAIN",null,null,null,"84"]