**SFN 1800930**

**CUY-6-1456**

**LEFT SIDE OF TOWER**

September 2010 inspection measurement was 3.5”.

March 2011 inspection the measurement was 3 5/8”.

**RIGHT SIDE OF TOWER**

September 2010 inspection measurement was 2 15/16”.

March 2011 inspection measurement was 3 1/16”.

Crack gage was installed in 2006 and was at 0 mm.

In 2007 the gage was at 9 mm.

2008 and 2009 B & N did the inspections so there is no measurement of how much the crack gage moved.

In September 2010 the crack gage was at 35 mm.

In March 2011 the crack gage was at 37 mm.