3

MAINT RESP 1 OHIO TRAN DEPT

PERCENT LEGAL = 150

SIGNS ON = N

MVC on = 9999.0

UNDER C = 0

UNDER NC = 0

1

8 SLIGHT CHANCE OVERTOPPING

3 Solid Wall

2 CANTILEVER

ABUTMENT NOT ON PILING

4 OPEN COLUMN

PIERS NOT ON PILING

1 Rollers

PAINT DATE 3/4/2004 5 PAINT SYSTEM OZE

15 Rolled Steel

1

1

1

1

1

1801503

3 LATEX MODIFIED CONCRETE OVERLAY

THK 1.2

 Lanes on 8

 3 SCUPPERS & DWNSPTS

6

1

2

1

2

1

1

1

2

7

3

5

1

1

1

3

2

6

DIVE DATE 10/15/2010

CULVERT FILL DEPTH = 0

2

3 SHEET PILING

6

8

 5 A

WRW

69991

12/30/2010

12/30/2010

ADK

N

1

1

1

0 OTHER

8 BITUMINOUS

1

1

2

CULVERT LENGTH = 0

N NONE/NOT APPLICABLE

N NONE – NATURAL PROTECTION

4

SPANS = 20

PIERS = 15 03 01

1

2

1

S

2

2

2

2

1

MAX SPANS 299

0 OTHER

2

5 REINFORCED CONCRETE PARAPET

2

out/out 83 Deck Area 272,652 sqft

1 REINF CONC (PRESTRSD, PRECAST)

Left 2 SIDEWALK (>2’)/Right 2 SIDEWALK (>2’)

CUY RIVER VALLEY & FI RR

5 7

343

12

1932

CUY 00010 1613