**ITEM SPECIAL - ASBESTOS ABATEMENT**

An asbestos surveys was conducted on the Newell Street over SR-2 and was completed on XXXX XX, XXXX by a certified asbestos hazard evaluation specialist from XXXXXXX XXXX The survey identified the asbestos containing materials at the location listed in the chart below.

**Insert Attached Table**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Bridge** | **Description** | **SFN** | **ACM** | **Location** | **Amount to be removed**  |
| **LAK-2-14.28** | Newell Street over SR 2 | 4301358 | XXXXXX | XXXXXXX | XX square feet |

The removal and disposal of any asbestos containing material during the deck replacement of the bridge must comply with the Ohio Administrative Code, the Occupational Safety and Health Administration (OSHA) regulations, and the National Emission Standard for Hazardous Air Pollutants (NESHAP) Standards for Asbestos.

A copy of the Ohio Environmental Protection Agency (OEPA) Notification of Demolition and Renovation forms with sections I-IV, VI and VII completed is included with the bid package. The Contractor will complete sections V, VIII-XVIII of the form and submit the completed form to the Local Air Authority at least ten (10) days prior to reconstruction of the bridges. The Contractor will provide a copy of the completed form to the Engineer. The Local Air Authority is:

 Lake County Air Pollution Control

Attn: Bert Mechenbier

 33 Mill Street

 Painesville, Ohio 44077

The Contractor will provide an individual trained in the provisions of NESHAP that will be on-site during removal of the asbestos containing materials. In addition to the asbestos containing material identified in the Asbestos Survey Report, this individual will also, monitor any additional non-visible asbestos encountered within the project work limits.

The Contractor will furnish all labor, equipment, and materials necessary to complete, submit, and comply with the OEPA Notification form and to remove, transport, and dispose of the materials containing asbestos from within the project work limits. Payment of this work will be included in the bid Lump Sum price Item Special - Asbestos Abatement.

**Item Unit**

 **Item Special - Asbestos Abatement Lump/Sum**