MOE-7-2.21 (PID 109278)

**TREE REMOVAL IS NOT PERMITTED WITH THIS PROJECT**

A TREE IS DEFINED AS A LIVE, DYING, OR DEAD WOODY PLANT, WITH A TRUNK THREE INCHES OR GREATER IN DIAMETER AT HEIGHT OF 4.5 FEET ABOVE THE GROUND SURFACE, AND WITH MINIMUM HEIGHT OF 13 FEET. IF IT IS DETERMINED THAT A TREE OR A SMALL GROUP OF TREES MUST BE REMOVED, THE CONTRACTOR SHALL NOTIFY THE DISTRICT ENVIRONMENTAL COORDINATOR RACHEL GOODPASTER AT (740) 568-4391 SIXTY (60) DAYS BEFORE REMOVING TREES. ALL TREE REMOVAL SHALL OCCUR FROM OCTOBER 1 THROUGH MARCH 31. BECAUSE THE PROJECT IS LOCATED WITHIN THE KNOWN RANGES OF THE FEDERALLY LISTED AND PROTECTED INDIANA BAT AND NORTHERN LONG-EARED BAT, NO TREES SHALL BE REMOVED UNDER THIS PROJECT FROM APRIL 1 THROUGH SEPTEMBER 30.

**WASTE AND BORROW IS NOT PERMITTED WITHIN RIGHT-OF-WAY**

THE CONTRACTOR SHALL NOT WASTE OR BORROW ANYWHERE WITHIN ODOT RIGHT OF WAY UNDER THIS PROJECT.

**WETLAND AND STREAM AVOIDANCE**

WETLAND HABITATS HAVE BEEN IDENTIFIED EAST OF STATE ROUTE 7 BETWEEN STATIONS 149+00 AND 154+00 AT THE TOE-OF-SLOPE JUST WITHIN AND BEYOND EXISITNG RIGHT-OF-WAY. TO AVOID UNAUTHORIZED WETLAND IMPACTS, NO CONSTRUCTION ACTIVITIES OR ANCILLARY CONSTRUCTION (STAGING AREAS, WASTE LOCATIONS, AND/OR BORROW LOCATIONS) ARE PERMITTED BEYOND THE TOE-OF-SLOPE AND RIGHT-OF-WAY LIMITS IN THE AREA DEFINED ABOVE.

WETLAND HABITATS HAVE BEEN IDENTIFIED EAST OF STATE ROUTE 7 BETWEEN STATIONS 251+50 AND 252+50 IMMEDIATELY BEYOND EXISITNG RIGHT-OF-WAY. TO AVOID UNAHUTHORIZED WETLAND IMPACTS, NO CONSTRUCTION ACTIVITIES OR ANCILLARY CONSTRUCTION (STAGING AREAS, WASTE LOCATIONS, AND/OR BORROW LOCATIONS) ARE PERMITTED BEYOND THE TOE-OF-SLOPE AND RIGHT-OF-WAY LIMITS IN THE AREA DEFINED ABOVE.

WETLAND HABITATS HAVE BEEN IDENTIFIED EAST OF STATE ROUTE 7 BETWEEN STATIONS 266+50 AND 269+50 IMMEDIATELY BEYOND THE EXISITNG ROADWAY DRAINAGE DITCH. TO AVOID UNAHUTHORIZED WETLAND IMPACTS, NO CONSTRUCTION ACTIVITIES OR ANCILLARY CONSTRUCTION (STAGING AREAS, WASTE LOCATIONS, AND/OR BORROW LOCATIONS) ARE PERMITTED BEYOND THE TOE-OF-SLOPE AND RIGHT-OF-WAY LIMITS IN THE AREA DEFINED ABOVE.

AN UNNAMED TRIBUTARY TO PATTON RUN (STREAM 2) HAS BEEN IDENTIFIED ON THE RIGHT OF WAY SHEET AT THE CULVERT AT STATION 424+75. AT THE PIPE OUTLET THE STREAM FLOWS NORTHEAST WITHIN THE EXISTING DRAINAGE DITCH. TO AVOID UNAUTHORIZED IMPACTS, NO CONSTRUCTION ACTIVITES OR ANCILLARY CONSTRUCTION (STAGING AREAS, WASTE LOCATIONS, AND/OR BORROW LOCATIONS) ARE PERMITTED WITHIN THE EXISTING DRAINAGE DITCH DEFINED ABOVE. ONLY IMPACTS ASSOCIATED WITH THE CULVERT REPLACEMENT ARE PERMITTED WITHIN THIS AREA AND SHOULD NOT EXTEND MORE THAN 20 FEET ALONG THE DRAINAGE DITCH IN A NORTHEAST DIRECTION FROM THE CULVERT OUTLET.