Conduit Inventory - Active & V - Village Maintained (Editor): 2001550

NLFID	CLICCR00003**C
CRS	LIC-3-5.788
ODOT District	05
County	LICKING
County CD	LIC
Route Type	County Road
Route Number	00003
Route Suffix	
CTL Begin Number	5.788
STL Begin Number	
Latitude DD Begin	40.241925
Longitude DD Begin	-82.688596
Perp Date	12/30/25
Status	Active
Installation Date	1/1/30
Let Plans URL	
Special Designation (Formerly Road ID)	Mainline
Conduit File Number (CFN)	2001550
Replacing Conduit	No
CFN of Replaced Conduit	
Legacy CFN	
Conduit Owner	V - Village
Maintenance Responsibility	V - Village
Entry Class	Class C (Alternate Entry Permit Required)
Feature Intersected	
Number of Cells	1
Broken Back	No
Conduit Shape	Slab Top Conduit
Conduit Material	Stone
Span (Inches)	48
Rise (Inches)	60
Length (Feet) (Include extensions)	30
Metal Gauge Thickness	
Type of Pipe Protection	Unprotected
Slope of Pipe (Percent)	
Skew (Degrees)	0
Centerline Span	48
Inlet End Treatment	Full Height Concrete Headwall
Outlet End Treatment	Full Height Concrete Headwall
Closed System	N
Maximum Height of Cover (Feet)	5
Scour Critical	No
Height of Inlet Headwall (Feet)	11
Inlet Headwall to Edge Pavement Distance (Feet)	
Height of Outlet Headwall (Feet)	11
Outlet Headwall to Edge Pavement Distance (Feet)	
Headwall Critical	No
Atmospheric or Physical Hazard	No
Drainage Area (Acres)	
Drainage Discharge (CFS)	
Abrasion Level (Set to 1 for Nonabrasive)	Level 2
pH	
Conduit Media	\\filestore.dot.state.oh.us\Conduits_Inspection\D05\LICKING\CR\3\2001550
Inventory Comments	Cut sandstone abutment walls - 23’ long with concrete abutment wall extension - 7’.

Cut sand stone slabs as top slab.

No mortar in joints, Dry joint construction.
Modification Type	
Year Modified	
Modification Comments	
PID	
Capital FY	
Latest GA	3
Latest Inspection Date	4/21/26, 2:17 PM
Year of Last Inspection	2026
Frequency Year	1
Latest Level of Inspection	Manned entry inspection
Inspection Due	
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