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SNBI SCOUR APPRAISAL NOTES
SNBI SCOUR APPRAISAL NOTES
Bridge: BEL-001SP-0051 	SFN: 0726184

1. Scour Evaluation Documentation
‘No’, move on to Section 3.

3.	Scour Assessment Level 1 – Stability Screening.
Countermeasure Type
Coded as ‘4 – none’ based on most recent plans and inspection photos.  RCP along abutments only.       
(1) Does the Bridge have unknown foundations?
Coded as No, as plans are available.
(2) Is there Visibly scoured Rock?
Coded as No. Previous inspection comments note scour (deterioration of piles, flaking of piles, etc), but such issues were resolved in 2022.      
(3) Shallow Foundations?
Coded as No, as substructure is on piles. 
(4) Evidence of History of Overtopping?
Coded as No, as OHHWM is below bridge deck elevation (only water mark available in plans). 
(5) Are any of, Scour, Channel, channel protection or underwater inspections coded 5 or worse?
No

A – Bridge is Stable for Scour

· Fill out Section 2. Scour Assessment Documentation. 
· Fill out Excel Tracker
· Select Correct Code under B.AP.03 Scour Vulnerability Code
· Form is now complete.
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